MyHealth@Eu MVC package
9.1.0 - trial-use

MyHealth@Eu MVC package - Local Development build (v9.1.0) built by the FHIR (HL7® FHIR® Standard) Build Tools. See the Directory of published versions

## ValueSet: eHDSI Technical Modality

Official URL: http://terminology.ehdsi.eu/ValueSet/eHDSITechnicalModality | Version: 9.1.0
Active as of 2026-05-07 | Computable Name: EHDSITechnicalModality
Other Identifiers: OID:1.3.6.1.4.1.12559.11.10.1.3.1.42.99

The Value Set is used for identifing the type of equipment, or function or technique of that equipment, that created the data used to create an instance, other than by means of acquisition through interaction with a patient or specimen.

References

This value set is not used here; it may be used elsewhere (e.g. specifications and/or implementations that use this content)

### Logical Definition (CLD)

- Include these codes as defined in `http://dicom.nema.org/resources/ontology/DCM` version 📍2022.4.20221006

  Code | Display | Definition
  `ASMT` | Content Assessment Result | A device, process or method that produces assessments of the content of other instances, e.g., for quality or suitability.
  `AU` | Audio | An acquisition device, process or method that records audio.
  `CTPROTOCOL` | CT Protocol | A device, process or method that produces CT device acquisition protocols.
  `DOC` | Document | A device, process or method that produces documents. i.e., representations of documents as images, whether by scanning or other means.
  `FID` | Spatial Fiducials | A device, process or method that identifies features or landmarks used to establish spatial correlation between objects or frames of reference.
  `HC` | Hard Copy | A device, process or method that creates images to be printed as hard copy.
  `IOL` | Intraocular Lens Calculation | A device, process or method that encodes calculations for an intraocular lens.
  `KO` | Key Object Selection | A device, process or method that creates Key Object Selection objects.
  `M3D` | 3D Manufacturing Modeling System | A device, process or method that produces data (models) for use in 3D manufacturing.
  `OT` | Other Modality | Other Modality device.
  `PLAN` | Plan | A device, process or method that produces treatment plans, e.g., delivery instructions for RT.
  `PR` | Presentation State | A device, process or method that creates Presentation State objects.
  `REG` | Registration | An image processing device, process or method that creates Registration objects.
  `RTDOSE` | Radiotherapy Dose | A device, process or method that records radiotherapy dose.
  `RTPLAN` | Radiotherapy Plan | A device, process or method that produces radiotherapy plans.
  `RTRECORD` | Radiotherapy Treatment Record | A device, process or method that records radiotherapy treatment records.
  `RTSTRUCT` | Radiotherapy Structure Set | A device, process or method that produces Radiotherapy Structure Sets.
  `RWV` | Real World Value Map | A device, process or method that produces mappings between image pixel values and some real-world values.
  `SEG` | Segmentation | An image processing device, process or method that performs segmentation.
  `SMR` | Stereometric Relationship | A device, process or method that records relationships between stereometric image pairs.
  `SR` | Structured Report Document | A device, process or method that creates Structured Report documents.
  `STAIN` | Automated Slide Stainer | A device, process or method that applies, in an automated manner, a stain, or reagent, to microscopy slides in preparation for imaging.
  `TEXTUREMAP` | Texture Map | A device, process or method that produces texture maps.

### Expansion

Expansion performed internally based on codesystem DICOM v2022.4.20221006 (CodeSystem)

This value set contains 23 concepts

System | Code | Display (en) | Definition | JSON | XML
`http://dicom.nema.org/resources/ontology/DCM` | `ASMT` | Content Assessment Result | A device, process or method that produces assessments of the content of other instances, e.g., for quality or suitability. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `AU` | Audio | An acquisition device, process or method that records audio. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `CTPROTOCOL` | CT Protocol | A device, process or method that produces CT device acquisition protocols. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `DOC` | Document | A device, process or method that produces documents. i.e., representations of documents as images, whether by scanning or other means. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `FID` | Spatial Fiducials | A device, process or method that identifies features or landmarks used to establish spatial correlation between objects or frames of reference. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `HC` | Hard Copy | A device, process or method that creates images to be printed as hard copy. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `IOL` | Intraocular Lens Calculation | A device, process or method that encodes calculations for an intraocular lens. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `KO` | Key Object Selection | A device, process or method that creates Key Object Selection objects. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `M3D` | 3D Manufacturing Modeling System | A device, process or method that produces data (models) for use in 3D manufacturing. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `OT` | Other Modality | Other Modality device. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `PLAN` | Plan | A device, process or method that produces treatment plans, e.g., delivery instructions for RT. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `PR` | Presentation State | A device, process or method that creates Presentation State objects. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `REG` | Registration | An image processing device, process or method that creates Registration objects. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `RTDOSE` | Radiotherapy Dose | A device, process or method that records radiotherapy dose. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `RTPLAN` | Radiotherapy Plan | A device, process or method that produces radiotherapy plans. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `RTRECORD` | Radiotherapy Treatment Record | A device, process or method that records radiotherapy treatment records. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `RTSTRUCT` | Radiotherapy Structure Set | A device, process or method that produces Radiotherapy Structure Sets. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `RWV` | Real World Value Map | A device, process or method that produces mappings between image pixel values and some real-world values. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `SEG` | Segmentation | An image processing device, process or method that performs segmentation. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `SMR` | Stereometric Relationship | A device, process or method that records relationships between stereometric image pairs. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `SR` | Structured Report Document | A device, process or method that creates Structured Report documents. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `STAIN` | Automated Slide Stainer | A device, process or method that applies, in an automated manner, a stain, or reagent, to microscopy slides in preparation for imaging. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `TEXTUREMAP` | Texture Map | A device, process or method that produces texture maps. |  |

Explanation of the columns that may appear on this page:

Level | A few code lists that FHIR defines are hierarchical - each code is assigned a level. In this scheme, some codes are under other codes, and imply that the code they are under also applies
System | The source of the definition of the code (when the value set draws in codes defined elsewhere)
Code | The code (used as the code in the resource instance)
Display | The display (used in the display element of a Coding). If there is no display, implementers should not simply display the code, but map the concept into their application
Definition | An explanation of the meaning of the concept
Comments | Additional notes about how to use the code